FIELDPIX
Pre-drywall inspection checklist
fieldpix.org/guides/pre-drywall-inspection-checklist
Job / address: ______________________________
Walked by: ______________________________
Date: ______________________________
With: ______________________________
Before you start
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Plans, electrical layout and selections on hand
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Rough inspections passed (framing, electrical, plumbing, mechanical)
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Insulation not yet installed
	☐ OK  ☐ Fix  ☐ N/A
	
	


Framing
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Studs straight and plumb, nothing split or cracked
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Headers over every window and door
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Window and door openings sized for the units ordered
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Notches and holes within limits, or repaired
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Hangers, straps and hold-downs fully nailed
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Blocking for cabinets, grab bars, TV, handrails and towel bars
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Fireblocking where required
	☐ OK  ☐ Fix  ☐ N/A
	
	

	No water stains on sheathing or roof deck
	☐ OK  ☐ Fix  ☐ N/A
	
	


Electrical
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Every box where the plans put it, at the planned height
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Boxes set out for the finished wall (thicker for tile)
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Cables stapled, not crushed, nail plates where needed
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Dedicated circuits for appliances
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Outlets for counters, island and exterior walls
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Low voltage: data, TV, doorbell, cameras, speakers
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Smoke and CO detector locations
	☐ OK  ☐ Fix  ☐ N/A
	
	


Plumbing and gas
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Supply and drains placed for the fixtures ordered
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Toilet distance from the wall
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Shower valve and head heights
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Tub and shower set, level and protected
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Pressure test passed, no drips or stains
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Nail plates where pipes are close to the stud face
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Gas lines capped and tested
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Washer box, ice maker line and hose bibs
	☐ OK  ☐ Fix  ☐ N/A
	
	


Heating, cooling and ventilation
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Ducts connected, sealed and supported
	☐ OK  ☐ Fix  ☐ N/A
	
	

	No crushed or kinked flex duct
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Registers and returns where planned
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Bath fans, range hood and dryer vented outside
	☐ OK  ☐ Fix  ☐ N/A
	
	


Photos
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Every wall of every room, floor to ceiling
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Tape measure in the frame at a known height
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Corners and ceilings
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Photos labeled by room
	☐ OK  ☐ Fix  ☐ N/A
	
	


Sign-off
	Check
	OK / Fix / N/A
	Notes
	Photo #

	Fix items on a punch list with who and when
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Fix items re-checked
	☐ OK  ☐ Fix  ☐ N/A
	
	

	Cleared for insulation and drywall
	☐ OK  ☐ Fix  ☐ N/A
	
	


Free template from fieldpix.org. FieldPix can write this for you from a walkthrough on site.




